|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Transaction** | **Method** | **Transaction Type** | **Schema with Extension** | |
| N/A | NA\_1 | Generic | WCTP-1.3 | ACM-v1r2 |
| [PCD-06] | PCD\_06\_1 | No MCR | WCTP-1.3 |  |
| [PCD-06] | PCD\_06\_2 | Unpaired MCR | WCTP-1.3 |  |
| [PCD-06] | PCD\_06\_3 | Paired MCR with No Additions | WCTP-1.3 |  |
| [PCD-06] | PCD\_06\_4 | Paired MCR with Callback | WCTP-1.3 | ACM-v1r1 |
| [PCD-06] | PCD\_06\_5 | Paired MCR with WCM | WCTP-1.3 | ACM-v1r1 |
| [PCD-06] | PCD\_06\_6 | Paired MCR with Alert Information | WCTP-1.3 | ACM-v1r2 |
| [PCD-06] | PCD\_06\_7 | Paired MCR with Callback and WCM | WCTP-1.3 | ACM-v1r1 |
| [PCD-06] | PCD\_06\_8 | Paired MCR with Callback and Alert Information | WCTP-1.3 | ACM-v1r2 |
| [PCD-06] | PCD\_06\_9 | Paired MCR with WCM and Alert Information | WCTP-1.3 | ACM-v1r2 |
| [PCD-06] | PCD\_06\_10 | Paired MCR with Callback, WCM, and Alert Information | WCTP-1.3 | ACM-v1r2 |
| [PCD-07] | PCD\_07\_1 | Synchronous Status Update with Success | WCTP-1.3 |  |
| [PCD-07] | PCD\_07\_2 | Synchronous Status Update with Failure | WCTP-1.3 |  |
| [PCD-07] | PCD\_07\_3 | Asynchronous Status Update | WCTP-1.3 |  |
| [PCD-07] | PCD\_07\_4 | Asynchronous Response with MCR | WCTP-1.3 |  |
| [PCD-07] | PCD\_07\_5 | Asynchronous Status Update with Alert Information | WCTP-1.3 | ACM-v1r2 |
| [PCD-07] | PCD\_07\_6 | Asynchronous Response with MCR and Alert Information | WCTP-1.3 | ACM-v1r2 |